For 1990-2009 cars

### Removal Procedure

Notice: Do not use solvent of any type when cleaning the gasket surfaces on the intake manifold and the throttle body assembly, as damage to the gasket surfaces and throttle body assembly may result.

Use care in cleaning the gasket surfaces on the intake manifold and the throttle body assembly, as sharp tools may damage the gasket surfaces.

Notice: Do not use any solvent that contains Methyl Ethyl Ketone (MEK). This solvent may damage fuel system components.

1. Turn OFF the ignition.
2. Remove the air cleaner outlet resonator. Refer to Air Cleaner Outlet Resonator Replacement .
3. Disconnect the idle air control (IAC) valve harness connector.
4. Disconnect the throttle position (TP) sensor harness connector.
5. Remove the vacuum hoses from the throttle body.
6. Remove the accelerator cable. Refer to Accelerator Control Cable Replacement .
7. Remove the cruise control cable, if applicable.
8. Remove the accelerator cable bracket. Refer to Accelerator Control Cable Bracket Replacement .
9. Remove the throttle body attaching bolts (1).
10. Remove the manifold absolute pressure (MAP) sensor.
11. Remove the throttle body from the intake manifold.

### Installation Procedure

Notice: The EVAP canister may have released carbon particles which caused this part to fail and may cause damage to other components. Check the EVAP canister for loose carbon before returning the vehicle to service.

1. Install the throttle body (3).
2. Install the accelerator cable bracket (2). Refer to Accelerator Control Cable Bracket Replacement .
3. Install the MAP sensor.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the MAP sensor bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

5. Install the throttle body attaching bolts (1).

Tighten
Tighten the bolts to 10 N·m (89 lb in).

6. Reinstall the accelerator cable to the throttle body. Refer to Accelerator Control Cable Replacement .
7. Install the cruise control cable, if applicable.
8. Install the vacuum hoses to throttle body.
9. Connect the IAC valve harness connector.
10. Connect the TP sensor harness connector.
11. Connect the air cleaner outlet resonator. Refer to Air Cleaner Outlet Resonator Replacement .

Important: With the engine OFF, inspect to see that the accelerator pedal moves freely by pressing the pedal to the floor and releasing.

12. Reconnect the negative battery cable.
13. Reset the IAC valve pintle position:

13.1. | Turn ON the ignition, with the engine OFF.

13.2. | Turn OFF the ignition for 10 seconds.

13.3. | Start the engine and verify the correct idle operation.