Electrical Connector and Manual Valve Assemble. Chevrolet Beretta 1996

For 1990-2009 cars

1. Inspect the manual valve (406) for damage.
2. Insert the manual valve (406) into the case cover (401) as shown. Be careful not to insert the valve backward.
3. Inspect the manual valve (406), and determine that the valve moves freely in the case cover bore.
4. Install the O-ring (407) onto the electrical connector (408).
5. Install the electrical connector into the case cover (401).