Cylinder Head Installation. Chevrolet Beretta 1996

For 1990-2009 cars

#### Tools Required

J 36660-A Torque Angle Meter.

Important: Install the cylinder head gasket with the words THIS SIDE UP showing.

1. Install the cylinder head gasket to the block.
2. Use a socket in order to push the cylinder head gasket over the rear dowel pin.
3. Carefully guide the cylinder head into place over the dowel pins. This operation may require an assistant.
4. Install the cylinder head bolts by hand.

Important: Use J 36660-A in order to tighten all the cylinder head bolts an additional 90 degrees in sequence.

5. Use the following sequence in order to tighten the cylinder head bolts:

Tighten

1. Tighten bolt 1 to 63 N·m (46 lb ft).
2. Tighten bolt 2 to 58 N·m (43 lb ft).
3. Tighten bolt 3 to 58 N·m (43 lb ft).
4. Tighten bolt 4 to 63 N·m (46 lb ft).
5. Tighten bolt 5 to 63 N·m (46 lb ft).
6. Tighten bolt 6 to 58 N·m (43 lb ft).
7. Tighten bolt 7 to 58 N·m (43 lb ft).
8. Tighten bolt 8 to 63 N·m (46 lb ft).
9. Tighten bolt 9 to 63 N·m (46 lb ft).
10. Tighten bolt 10 to 58 N·m (43 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the engine lift bracket(s) onto the front and the rear of the engine.