BROKEN DOOR HOLD OPEN CHECK LINK (REPLACE CHECK LINK). Chevrolet Beretta 1987

For 1990-2009 cars

# BROKEN DOOR HOLD OPEN CHECK LINK (REPLACE CHECK LINK)

#### Model and Year: 1987-88 BERETTA, CORSICA

Broken door hold open check links on the above listed vehicles may be repaired by replacing the component with a new check link.

New parts are available from GMSPO and the part numbers are as follows:

Beretta - P/N 10124201

Corsica Front - P/N 10124270

Rear - P/N 10124271

Labor Operation Time --------------- ---- Front B4050 - Right .2 Hours B4051 - Left .2 Hours

Rear B4450 - Right .5 Hours B4451 - Left .5 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.