REAR SPEAKER ASSEMBLY FALLS OUT OF MOUNT. Chevrolet Beretta 1988

For 1990-2009 cars

# REAR SPEAKER ASSEMBLY FALLS OUT OF MOUNT

#### VEHICLES AFFECTED: 1987-88 'L' CARS

Some vehicles have had rear speaker assemblies falling off of their mountings on the rear compartment shelf. This occurs when the tabs on the speaker assembly come out of their slots in the rear seat to the back window panel.

To repair this condition install an I/P trim plate clip, P/N 25510099, on each of the speaker enclosure tabs and reinstall the assembly. See Illustration.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim .2 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.