LOW COOL LIGHT/ACCEL. OR BRAKE DISCONNECT LOW COOL MODULE. Chevrolet Beretta 1987

For 1990-2009 cars

# LOW COOL LIGHT/ACCEL. OR BRAKE DISCONNECT LOW COOL MODULE

#### VEHICLES AFFECTED: 1987 'L' CARS WITH LB6 2.8L V6 ENGINES (VIN CODE W)

Some vehicles may exhibit an intermitent low coolant light on acceleration or braking conditions, when coolant is not low. This condition can be repaired by disconnecting the low coolant module, under the dash and taping the lead to wiring harness, as shown in Illustrations.

The following breakpoints are VIN numbers of vehicles that have already been repaired at the assembly plant.

Wilmington - Y 100691

Linden - E 104528

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.