Engine Flywheel Installation. Chevrolet Beretta 1996

For 1990-2009 cars

1. Install the flywheel.
2. Install the flywheel retainer.
3. Install the flywheel bolts.

Tighten
Tighten the bolts to 83 N·m (61 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the exhaust crossover pipe.
5. Install the exhaust crossover pipe retaining nuts.

Tighten
Tighten the nuts to 25 N·m (18 lb ft).

6. Install the exhaust crossover pipe heat shield.
7. Install the exhaust crossover pipe heat shield screws.

Tighten
Tighten the screws to 10 N·m (89 lb in).