SMU - SECTION 6B - ADDITIONAL INFORMATION. Chevrolet Beretta 1995

For 1990-2009 cars

# SMU - SECTION 6B - ADDITIONAL INFORMATION

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6B - ADDITIONAL INFORMATION TO STEP 3 OF "FILLING THE COOLING SYSTEM" PROCEDURE

#### MODELS: 1995 CHEVROLET BERETTA, CORSICA WITH 2.2L ENGINE (VIN 4 - RPO LN2)

PLEASE ADD THE FOLLOWING INFORMATION TO STEP 3 OF THE "FILLING" PROCEDURE FOUND ON PAGE 6B-10 OF THE SERVICE MANUAL:

#### IMPORTANT:

ON VEHICLES PRODUCED WITH THE 2.2L ENGINE, LOOSEN THE ENGINE COOLANT AIR BLEED SCREW LOCATED ON THE TOP SIDE OF THE ENGINE COOLANT OUTLET. ADD COOLANT UNTIL ALL AIR IS EVACUATED THROUGH AIR BLEED. TIGHTEN AIR BLEED SCREW. REFER TO FIGURE 13 ON PAGE 6B-12 FOR COOLANT BLEED LOCATION.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.