DELCO CS SERIES GENERATOR EXCHANGE PROGRAM AND P/N'S. Chevrolet Beretta 1987

For 1990-2009 cars

# DELCO CS SERIES GENERATOR EXCHANGE PROGRAM AND P/N'S

#### MODEL AND YEAR: SELECT 1987 PASSENGER CARS AND LIGHT DUTY TRUCKS

The Delco CS series generators will be used in a wide variety of models and applications for the 1987 model year. To aid in the analysis of field returned parts, Delco Remy and Chevrolet have instituted an exchange program for the 1987 model year.

When in-dealership diagnosis indicates an internal generator problem, obtain the appropriate replacement generator from GMWDD using the Order Exchange Part Number listed below. Service parts for in-dealership repair of these CS generators will not be available. Properly complete the return tag, which will be supplied with the exchange generator, and attach it to the removed generator. Package the removed generator in the replacement generator box and return to GMWDD for credit; otherwise, a $17.00 core charge will result.

The following is a listing of CS generator applications for the 1987 model year which are included in this exchange program. Unlisted models and/or applications are not included in this exchange proGram, and normal repair procedures apply.

#### PASSENGER CAR

Original Equipment Order Exchange Model Engines Amps Part Number Part Number ----- ------- ---- ------------------ -------------- Celebrity 2.5L 85 1101142 10463016 2.8L 85 1101135 10463009 l00 1101136 10463010

Camaro 2.8L 85 1101139 10463013 l00 1101140 10463014 5.0L 85 1101137 10463011 l00 1101138 10463012 5.0L PFI 105 1101141 10463015 5.7L PFI 105 1101141 10463015

Cavalier 2.0L 74 1105697 10456312 85 1105701 10463043 2.8L 85 1105698 10463042 l00 1105694 10463040

Corvette 5.7L PFI 105 1101127 10463007

Corsica/ 2.0L 74 1105697 10456312 Beretta 85 1105701 10463043 2.5L 85 1105698 10463042 l00 1105694 10463040

#### LIGHT DUTY TRUCK

Original Equipment Order Exchange Model Engines Amps Part Number Part Number ----- ------- ---- ------------------ --------------

C,K,G VAN 4.3L 85 1105710 10463044 (EX. SUB) l00 1105711 10463045 5.0L 85 1105710 10463044 l00 1105711 10463045 5.7L 85 1105710 10463044 l00 1105711 10463045

(EX. G VAN) 6.2LD 85 1101110 10463044 l00 1101111 10463045 7.4L 85 1105712 10497077 l00 1105688 10463039

M VAN 2.5L 85 1105722 10463049 4.3L 85 1105710 10463044 l00 1105711 10463045

P VAN 5.7L 85 1105718 10463047 105 1105720 10463048 7.4L 105 1105661 10463038

SUB 5.0L 105 1105720 10463048 5.7L 105 1105720 10463048 7.4L 105 1105661 10463038 S/T 2.5L 85 1105722 10463049 2.BL 85 1101259 10463034

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.