Valve Rocker Arm, Push Rod, and Stud Installation. Chevrolet Beretta 1996

For 1990-2009 cars

Important: When you install new rocker arms and new rocker arm balls, coat the mating surface with Camshaft Assembly Lubricant (GM P/N 1052365) or equivalent.

1. Install the pushrods.

Make sure that the pushrods seat in the lifters.

2. Install the rocker arms.
3. Install the rocker arm balls.

Important: Do not over tighten the rocker arm nuts.

4. Install the rocker arm nuts.

Tighten
Tighten the rocker arm nuts to 30 N·m (22 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. The valve lifter should sit on the base circle of the camshaft.
6. Install the rocker arm cover. Refer to Valve Rocker Arm Cover Installation.