SMU-SEC. 1B REVISED FASTENER TORQUE FOR A/C COMPRESSOR. Chevrolet Beretta 1994

For 1990-2009 cars

# SMU-SEC. 1B REVISED FASTENER TORQUE FOR A/C COMPRESSOR

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 1B - REVISED FASTENER TORQUE FOR A/C COMPRESSOR AND COMPRESSOR BRACKET

#### MODELS: 1994 CHEVROLET CORSICA, BERETTA, CAVALIER WITH 2.2L ENGINE (VIN 4 - RPO LN2)

THE FOLLOWING TORQUE REVISIONS ARE TO BE INCLUDED IN SECTION 1B OF THE SERVICE MANUALS:

BOLT, A/C COMPRESSOR TO BRACKET . . . . . . . . . 47 N.M (35 LBS. FT.)

BOLT, A/C COMPRESSOR BRACKET TO ENGINE BLOCK. . . 47 N.M (35 LBS. FT.)

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.