No Drive in Forward Ranges. Chevrolet Beretta 1996

For 1990-2009 cars

Checks | Cause
--- | ---
Driven Sprocket Support (602) | The sleeve is turned (601)
Oil Pressure | See causes of low oil pressure
Manual Linkage (701-704) | The manual valve is not moving (406)

Driven Sprocket Support

• | The drive oil passage is blocked in the driven sprocket support or the gasket

• | The sleeve is loose or is mislocated (601)

Case Cover (401) | A leak exists in the drive oil passage
Forward Clutch (624-634) | Plates are burned or damaged (625, 633, 634)
Control Valve Assembly (21) | The valve body pipe is leaking or missing (370)