MANUAL UPDATE- REAR SUSPENSION NEW MOUNTING BOLT TORQUE. Chevrolet Beretta 1989

For 1990-2009 cars

# MANUAL UPDATE- REAR SUSPENSION NEW MOUNTING BOLT TORQUE

#### Model and Year: 1987-90 L CAR

Rear shock absorber mounting bolt torque is incorrectly listed in the Service Manual. This may cause a shock absorber rattle. Whenever installing the rear shock absorber, torque the lower mounting bolt to 47 N.m (35 lb. ft.).

Please update your Service Manuals.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.