Auxiliary Valve Body and Oil Pump Disassemble. Chevrolet Beretta 1996

For 1990-2009 cars

1. Remove the auxiliary valve body cover (330) and the auxiliary valve body assembly (343) from the control valve and oil pump assembly (21).
2. Remove the auxiliary valve body cover (330) from the auxiliary valve body (343).
3. Remove the following parts from the control valve and oil pump assembly (21):

• | The pump vane ring (351)

• | The pump rotor (353)

• | Seven pump vanes (352)

4. Remove the retaining pin (304) for the pump priming spring.
5. Remove the pump spring retaining plug (358) and the spring (359).
6. Remove the following parts from the control valve and oil pump assembly (21):

• | The pump slide (348)

• | The fluid seal ring (346)

• | The fluid seal (347)