RATTLE/CLICK AT START-UP (SHIELD CONVERTER, NEW P/N). Chevrolet Beretta 1989

For 1990-2009 cars

# RATTLE/CLICK AT START-UP (SHIELD CONVERTER, NEW P/N)

1985-89 J CAR AND 1988-89 L CAR WITH 2.8L (VIN CODE W) Model and Year: ENGINE AND AUTOMATIC TRANSMISSION 1990 J, L, W CAR WITH 3.1 (VIN COD T) ENGINE AND AUTOMATIC TRANSMISSION

Owners of 1985 through early 1990 J-cars and 1988 through early 1990 L-cars equipped with 2.8L or 3.1L V6 engines with automatic transmission may notice a rattling or clicking noise coming from the engine compartment. This noise is more apparent when the engine is cold and usually goes away as the engine warms up.

The above noise may be due to the torque converter shield. This warped shield may interfere with the flywheel.

A torque converter shield currently used on the W-car has been released for use on the 2.BL and 3.1L J and L car. See Figure on next page.

#### Parts:

Shield, Converter (previous) P/N 10085217

Shield, Converter (New) P/N 10009088

Replace cover, use three of the existing bolts removed from the vehicle.

Parts are currently available from GMSPO.

Labor Operation Number: J1440

Labor Time: .3 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.