Fastener Tightening Specifications. Chevrolet Beretta 1996

For 1990-2009 cars

Application | N·m | Lb Ft | Lb In.
--- | --- | --- | ---
Battery Retainer Bolt | 18 | 13 | --
Commutator End Frame/Field Frame Assembly Through Bolts | 8.5 | -- | 75
Front Bracket to Generator Bolt (3.1L) | 25 | 18 | --
Front Bracket to Generator Nut (3.1L) | 50 | 37(2.2L) | --
Front Generator Bracket to Block Attaching Bolt (2.2L) | 50 | 37 | --
Generator (Upper) Front Mounting Bolt (2.2L) | 30 | 22 | --
Generator (Lower) Front Mounting Bolt (2.2L) | 50 | 37 | --
Generator Rear Mounting Bolt | 25 | 18 | --
Ignition Wire Harness Bracket Nut 3.1L | 13 | 10 | --
Ignition Wire Harness Retaining Bolt 3.1L | 25 | 18 | --
Negative Battery Cable Terminal Nut | 16 | 12 | --
Negative Battery to Transaxle Stud Nut | 25 | 18 | --
Battery Cable to Battery Bolt | 16 | 12 | --
Positive Battery Cable Terminal Nut | 20 | 15 | --
Positive Battery Cable to Generator Nut | 7.5 | -- | 65
Positive Battery Cable to Starter Solenoid Nut | 14 | -- | 124
Rear Brace to Generator Bolt (3.1L) | 25 | 18 | --
Rear Brace to Engine Nut (3.1L) | 25 | 18 | --
Rear Generator Bracket to Block Attaching Bolt (2.2L) | 85 | 63 | --
Rear Generator Bracket to Block Attaching Nut (2.2L) | 43 | 32 | --
Rear of Generator to bracket bolt (2.2L) | 30 | 22 | --
Solenoid Attaching Screws | 11 | -- | 95
Spark Plugs (2.2L) | 18 | 13 | --
Spark Plugs (3.1L) | 15 | 11 | --
Starter Field Lead to Solenoid Attaching Screw | 9.5 | -- | 84
Starter Lead Wire to Starter Solenoid S Terminal Nut | 2.5 | -- | 22
Starter Motor Brace to Starter Motor Nut (2.2L) | 10 | -- | 89
Starter Motor Bracket to Engine Bolt (2.2L) | 32 | 24 | --
Starter Motor to Engine Bolt (2.2L) | 43 | 32 | --
Starter Motor to Engine Bolt (3.1L) | 43 | 32 | --
Starter Motor Solenoid to the S Terminal Nut | 2.5 | -- | 22