I/P CUP HOLDER BINDING/STUCK REMOVE AND WASH HOLDER ASSY.. Chevrolet Beretta 1991

For 1990-2009 cars

# I/P CUP HOLDER BINDING/STUCK REMOVE AND WASH HOLDER ASSY.

#### SUBJECT: INSTRUMENT PANEL CUP HOLDER BINDING/STUCK (REMOVE AND WASH INSTRUMENT PANEL CUP HOLDER ASSEMBLY)

VEHICLES AFFECTED: 1991-82 CHEVROLET CORSICA AND BERETTA 1991 PONTIAC TEMPEST

#### Condition:

--------- Some owners of 1991-92 L-cars may comment on the operation of the Instrument Panel (I/P) cup holder as sticking or binding.

#### Cause:

----- Carbonated soft drinks or fruit juices spilled on the sliding surfaces of the tracks may inhibit free movement of the cup holder.

#### Correction:

---------- Free operation may be restored as follows:

1. Remove I/P cup holder screws.

2. Remove I/P cup holder - air outlet assembly.

3. Wash thoroughly with luke-warm water and mild hand or dish soap and air dry. Harsh, chlorinated or soaps containing grit should not be used.

4. Install cup holder.

5. Tighten screws to 2 N.m (17 in.lbs.).

For vehicles repaired under warranty use:

Labour Operation Number: C2085

Labour Time: .2 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.