Control Valve Body Assemble. Chevrolet Beretta 1996

For 1990-2009 cars

1. Install the 3-2 regulating control valve (356).
2. Install the 3-2 regulating control valve spring (355).
3. Install the valve retaining pin (307).
4. Install the pressure regulator valve (365).
5. Install the reverse regulator spring (364), and the throttle valve and reverse boost valve spring (360).
6. Install the reverse boost valve (363).
7. Install the throttle valve (369).
8. Install the throttle valve retaining pin (306).
9. Install the throttle valve spring (368) and plunger (367).
10. Install the throttle valve bushing (366).
11. Install the bushing retaining pin (304).
12. Install the line boost valve (303).
13. Install the line boost valve bore plug (302).
14. Install the bore plug retaining pin (305).
15. Install the pressure regulator bore plug (372).
16. Install the bore plug retainer (373).
17. Install the shift throttle valve (308).
18. Install the shift throttle valve spring (309).
19. Install the bore plug (310\382).
20. Install the retaining pin (304).
21. Install the pressure relief ball valve (311).
22. Install the ball valve spring (312).
23. Install the spring retaining pin (307).
24. Install the 1-2 accumulator valve spring (313).
25. Install the 1-2 accumulator bushing (314).
26. Install the 1-2 accumulator valve (315) and bore plug (310).
27. Install the 1-2 accumulator valve retainer (304).
28. Install the 2-3 shift valve (316) into the valve body.
29. Assemble the 2-3 throttle valve spring (318) and the throttle valve (317) into the 2-3 throttle valve sleeve (319).
30. Install the 2-3 throttle valve retainer (377) into the sleeve (319).
31. Install the 2-3 throttle valve and sleeve assembly (319) into the valve body.
32. Install the 2-3 throttle valve sleeve retaining pin (304).
33. Install the 1-2 shift valve (320) into the valve body.
34. Assemble the 1-2 throttle valve spring (322) and the 1-2 throttle valve (321) into the 1-2 throttle valve sleeve (323).
35. Install the 1-2 throttle valve retainer (377) into the throttle valve sleeve (323).
36. Install the 1-2 throttle valve and sleeve assembly (323) into the valve body.
37. Install the sleeve retainer (304).
38. Install the low blow off ball valve (324).
39. Install the low blow off valve seat and spring (325).
40. Install the low blow off valve plug (326).