Auxiliary Valve Body Disassemble. Chevrolet Beretta 1996

For 1990-2009 cars

1. On some models, remove the third clutch pressure switch (335).
2. Remove the governor pressure switch (338) (the second clutch switch on some models).
3. Remove the converter clutch control valve bore plug (310) and remove the control valve (332).
4. Remove the following parts:

• | The orifice control valve spring retainer (304)

• | The spring (381)

• | The valve (380)

5. Remove the auxiliary valve body filter (357).
6. Remove the auxiliary valve body sleeve (344).