Shifts 1-3, Misses Second Gear. Chevrolet Beretta 1996

For 1990-2009 cars

Checks | Cause
--- | ---

Intermediate Servo (128-137)

• | The apply pin is wrong or is sticking (129)

• | The seals are cut, are damaged, or are missing (128, 132, 134)

• | The piston is sticking or is damaged (133)

• | Porosity is in the case servo bore (15)

Accumulator Exhaust Valve (125-126) | The valve is sticking, not seating
Control Valve Assembly | The 1-2 shift valve is sticking (320)

Spacer Plate (20)

• | The gaskets are incorrectly installed (19)

• | The governor feed to the 1-2 shift valve is blocked

• | The intermediate band apply feed orifice is blocked (15, 137)

• | Wrong spacer plate

Case (15) | The intermediate servo apply passage (second oil) is blocked
Case Cover (40) | The intermediate servo apply passage (second oil) is blocked

Intermediate Band (606)

• | The band is improperly installed

• | The band is burned or broken