Slips in Reverse or No Reverse. Chevrolet Beretta 1996

For 1990-2009 cars

Checks | Cause
--- | ---

Direct Clutch (608-609)

• | Burned clutch plates

• | Seal ring is off the piston

• | Exhaust check ball is sticking

Lo and Reverse Clutch

• | Housing cup plug assembly is restricted or not fully seated

• | Leaking seals

Lo and Reverse Pipe | O-ring seal is damaged or missing

Case to Cover Gasket

• | Incorrect (the driven sprocket support height is wrong)

• | Damaged or leaking

Lo and Reverse Clutch | Burned plates
Manual Valve | A fallen out retainer clip
Low Line Pressure | Check the causes of low line pressure
Low Reverse Piston | Piston stuck