Oil Pump Removal. Chevrolet Beretta 1996

For 1990-2009 cars

1. Remove the oil pump drive bolt.
2. Remove the oil pump drive. Do this by lifting and turning the oil pump drive.

### Oil Pump Removal Procedure

1. Remove the oil pan. Refer to Oil Pan Removal.
2. Remove the bolt that attaches the oil pump to the rear main bearing cap.
3. Remove the oil pump.
4. Remove the oil pump drive shaft. Refer to Oil Pump Drive Removal

Important: Do not crack the oil pump drive shaft retainer.

5. Remove the oil pump drive shaft retainer.

Important: A loose oil pump tube can cause an air leak and a loss of oil pressure.

6. Inspect the oil pump pickup tube for looseness.