Drive Shaft Oil Seal Assemble - Right Side. Chevrolet Beretta 1996

For 1990-2009 cars

#### Tools Required

• | J 29130 Axle Seal Installer

• | J 8092 Driver

Notice: Install the seal onto the tool before installing into the case to prevent damage to the seal.

Important: Inspect the seal assembly to confirm that no damage has occurred. Confirm that the garter spring was not dislodged.

Using J 8092 and J 29130 , install the oil seal assembly (117) for the front wheel drive shaft onto the case.