W/S REVEAL MOLDING POOR FIT NEW MOLDING P/N AND REPAIR. Chevrolet Beretta 1988

For 1990-2009 cars

# W/S REVEAL MOLDING POOR FIT NEW MOLDING P/N AND REPAIR

#### Model and Year: 1987-88 BERETTA, CORSICA

Some comments have been made that the windshield side-to-pillar reveal moldings have a poor fit at the upper corners on subject vehicles.

Field repairs can be accomplished by installing a revised windshield side-to-pillar reveal molding per the service procedure below. The part numbers for the revised moldings are:

Coupe R/S 10076028 L/S 10076029

Sedan R/S 10076030 L/S 10076031

#### Service Procedure

1. Open front door.

2. Remove sealing strip in area of windshield side reveal molding.

3. Remove four screws, (see illustration).

4. If necessary, elongate the four holes and slots in the new reveal moldings so that the molding end will fit flush to the roof.

5. Install moldings and reverse the tear down procedure.

Labor Operation Labor Number Time

Right side, elongate B7570 .3 Hours holes, and replace.

Left side, elongate B7571 .3 Hours holes, and replace.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.