FRONT SEAT BACK TRIM COVER PULLS LOOSE-REPAIR DESCRIBED. Chevrolet Beretta 1988

For 1990-2009 cars

# FRONT SEAT BACK TRIM COVER PULLS LOOSE-REPAIR DESCRIBED

#### VEHICLES AFFECTED: 1988 BERETTA

Some cases of seat back trim pulling loose from the seat back on the 1988 Berettas may be reported. To repair this condition use the following procedure:

1. Remove front seat back head restraint and inertia lock knob as described in Section 9L-7 of the Corsica/Beretta Service Manual.

2. Remove seat back cover.

3. Drill a 3/16" hole through the "J" retainer and the metal frame as indicated on the Illustration.

4. Install self tapping screw, P/N 20365264 through "J" retainer into seat metal frame.

5. Reinstall seat head restraint, inertia lock knob, and seat back cover.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim 0.3 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.