SMU - SECTION 8A - REVISED MULTI-FUNCTION ALARM MODULE. Chevrolet Beretta 1996

For 1990-2009 cars

# SMU - SECTION 8A - REVISED MULTI-FUNCTION ALARM MODULE

REVISION: 10/02/95

THIS BULLETIN IS BEING REVISED TO CORRECT TEXT IN PARAGRAPH 1. PLEASE DISCARD BULLETIN 53-81-25 (GROUP REFERENCE 8 - CHASSIS/BODY ELECTRICAL). *********************************************************************

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 8A - REVISED MULTI-FUNCTION ALARM MODULE DIAGNOSTICS

#### MODELS: 1995 BUICK SKYLARK 1995-96 CHEVROLET BERETTA, CORSICA 1995 OLDSMOBILE ACHIEVA 1995 PONTIAC GRAND AM

WHEN PLACING THE MULTI-FUNCTION ALARM MODULE IN THE POWER OUTPUT DIAGNOSTIC MODE, 4 FAILURE MODES CAN BE SET. THE 1995 AND 1996 SERVICE INFORMATION DOES NOT LIST THE FOURTH FAILURE MODE AND SHOULD BE UPDATED AS FOLLOWS.

WHEN THE MULTI-FUNCTION ALARM MODULE CHIMES 4 TIMES EVERY 3 SECONDS DURING THE POWER OUTPUT DIAGNOSTIC MODE, A FAILURE OF THE SEAT BELT DOOR RETRACTOR SOLENOIDS HAS BEEN DETECTED AND THE APPROPRIATE DIAGNOSTIC CHART IN SECTION 8A-146 SHOULD BE REFERRED TO. ONCE THE NECESSARY REPAIRS HAVE BEEN PERFORMED, RESET THE MULTI-FUNCTION ALARM MODULE BY REMOVING FUSE 11 OR THE ALARM FUSE AS NOTED IN SECTION 8A-76.

THE PROCEDURE TO PLACE THE MULTI-FUNCTION ALARM MODULE IN THE POWER OUTPUT DIAGNOSTIC MODE IS LISTED IN SECTION 8A-76 BUT SHOULD ALSO BE ADDED TO SECTION 8A-146. THE PROCEDURE IS AS FOLLOWS:

1. CLOSE FRONT DOORS.

2. SET PARK BRAKE.

3. TURN INTERIOR LIGHTS ON USING PANEL DIMMER SWITCH.

4. TURN IGNITION SWITCH TO "RUN" AND BEFORE 15 SECONDS ELAPSE, PERFORM THE FOLLOWING STEPS:

A. OPEN RH FRONT DOOR. B. CYCLE HEADLAMP SWITCH FROM "PARK" TO "OFF" 3 TIMES.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.