Air Cleaner. Chevrolet Beretta 1996

For 1990-2009 cars

### Removal Procedure

1. Disconnect the air sensor electrical connector.
2. Remove the wing nuts from the air cleaner.
3. Place the wing nuts out of the way.
4. Remove the bolt from the air cleaner to the shock tower.
5. Separate the assembly from the intermediate duct and from the vehicle.

### Installation Procedure

1. Install the air cleaner assembly to the intermediate duct and the vehicle.
2. Install the air cleaner mounting bolt to the shock tower.
3. Install the air cleaner wing nuts.
4. Connect the intake air temperature sensor electrical connector.