RATTLES IN DOOR FROM SEAT BELT RETRACTORS (NEW RETRACTORS). Chevrolet Beretta 1989

For 1990-2009 cars

# RATTLES IN DOOR FROM SEAT BELT RETRACTORS (NEW RETRACTORS)

#### Model and Year: 1989 L CAR

THIS BULLETIN CANCELS AND SUPERSEDES DEALER SERVICE BULLETIN NO. 89-296-10, DATED FEBRUARY 1990. THE WORD WITHOUT COMFORT HAS BEEN CHANGED TO WITH COMFORT FOR THE 1989 LTV37 L CAR. ALL COPIES OF 89-296-10 SHOULD BE DISCARDED.

Owners of some 1989 Corsica and/or Berettas may comment on a rattle in the door caused by the seat belt retractor. New retractors have been released for production and service. The new retractors have been modified to eliminate rattles. New Part Numbers are:

1989 LT68 WITH COMFORT 1989 LTV37 WITH COMFORT

12502815-6 Med. Dk. Gray 12502823-4 Med. Dk. Gray 12502813-14 Garnet Red 12502821-2 Garnet Red 12502811-12 Black 12502819-20 Black 12502809-10 Very Dark Sapphire 12502817-18 Very Dark Sapphire 12503260-1 Beechwood

1989 LT68 - 69 WITHOUT COMFORT

12503258-9 Med. Dk. Gray 12503256-7 Garnet Red 12503254-5 Beechwood 12503252-3 Very Dark Sapphire

Parts are currently available from GMSPO.

Labor Operation Number: C9047 (Both Sides)

Labor Time: 1.5 Hours (Beretta Only)

Labor Operation Number: C9040 (Right) C9041 (Left)

Labor Time: .6 Hour (One Side) Corsica .8 Hour (One Side) Beretta

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.