Emission Hose Routing Diagram. Chevrolet Beretta 1996

For 1990-2009 cars

#### Emission Hose Routing Diagram - L 3100 (VIN M)

(1) | EVAP Vacuum Switch
(2) | EVAP Canister Purge Valve
(3) | To Rocker Arm Cover
(4) | Air Intake Duct
(5) | Throttle Body
(6) | PCV Valve
(7) | Fuel Pressure Regulator
(8) | To Transaxle/Accessory
(9) | Intake Manifold
(10) | To Top Port of EVAP Canister
(11) | EVAP Canister
(12) | To Fuel Tank
(13) | Capped
(14) | To Vacuum Brake Booster
(15) | MAP Sensor