Transmission Fluid Filler Tube and Seal Replacement. Chevrolet Beretta 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the oil level indicator.
2. Remove the nut or bolt that retains the fill tube to the mounting bracket.
3. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
4. Place a drain pan under the transmission.
5. Loosen the filler tube from the transmission.
6. Remove the filler tube seal.
7. Lower the vehicle.
8. Pull the tube out of the vehicle from the top.

### Installation Procedure

1. Install the filler tube through the top of the vehicle.
2. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
3. Install the filler tube seal into the transmission. Lubricate the seal with DEXRON®-IIE, or DEXRON®-III
4. Install the filler tube into the transmission.
5. Lower the vehicle.
6. Install the nut that retains the tube to the mounting bracket.
7. Install the oil level indicator.
8. Adjust the oil level.