Output Shaft, Reaction Gear, Low/Rev Clutch Removal. Chevrolet Brazil Blazer 1997

For 1990-2009 cars

#### Tools Required

J 29837 Output Shaft Support Fixture

1. Remove the following components: reaction sun gear; thrust washer; and the low/reverse roller clutch race.

1.1. | The reaction sun gear

1.2. | The thrust washer

1.3. | The low/reverse roller clutch race

2. Remove the low/reverse support retainer ring.
3. Push up on the output shaft in order to loosen the low/verse clutch support.
4. Remove the low/reverse clutch support.
5. Remove the transmission spring (low/reverse clutch support retainer).
6. Remove the reaction carrier assembly.
7. Remove the following components:

7.1. | The low/reverse clutch fiber plate assembly

7.2. | The low/reverse clutch steel plates

7.3. | The spacer

7.4. | The low/reverse clutch selective plate

7.5. | The low/reverse clutch waved plate

8. Remove the following components:

8.1. | The thrust bearing assembly (reaction carrier support)

8.2. | The internal reaction gear

8.3. | The internal reaction gear support

8.4. | The reaction gear support bearing

9. Remove the output shaft support fixture.
10. Remove the output shaft.