CAMPAIGN:WINDOW FOGGING. Chevrolet Brazil Blazer 1997

For 1990-2009 cars

# CAMPAIGN:WINDOW FOGGING

PRODUCT CAMPAIGNS 98031 AUGUST, 1998

PRODUCT RECALL CAMPAIGN

PRODUCT SAFETY CAMPAIGN

#### SUBJECT: 98031 - WINDOW FOGGING

#### MODELS: 1997-98 CHEVROLET S10 ELECTRIC TRUCK

THE HIGHWAY SAFETY ACT, AS AMENDED, PROVIDES THAT EACH VEHICLE WHICH IS SUBJECT TO A RECALL CAMPAIGN OF THIS TYPE MUST BE ADEQUATELY REPAIRED WITHIN A REASONABLE TIME AFTER THE CUSTOMER HAS TENDERED IT FOR REPAIR. A FAILURE TO REPAIR WITHIN SIXTY (60) DAYS AFTER TENDER OF A VEHICLE IS PRIMA FACIE EVIDENCE OF FAILURE TO REPAIR WITHIN A REASONABLE TIME.

IF THE CONDITION IS NOT ADEQUATELY REPAIRED WITHIN A REASONABLE TIME, THE CUSTOMER MAY BE ENTITLED TO AN IDENTICAL OR REASONABLY EQUIVALENT VEHICLE AT NO CHARGE OR TO A REFUND OF THE PURCHASE PRICE LESS A REASONABLE ALLOWANCE FOR DEPRECIATION.

TO AVOID HAVING TO PROVIDE THESE BURDENSOME REMEDIES, EVERY EFFORT MUST BE MADE TO PROMPTLY SCHEDULE AN APPOINTMENT WITH EACH CUSTOMER AND TO REPAIR THEIR VEHICLE AS SOON AS POSSIBLE. AS YOU WILL SEE IN READING THE ATTACHED COPY OF THE DIVISIONAL LETTER THAT IS BEING SENT TO CUSTOMERS, THE CUSTOMERS ARE BEING INSTRUCTED TO CONTACT THE APPROPRIATE CUSTOMER ASSISTANCE CENTER IF THEIR DEALER DOES NOT REMEDY THE CONDITION WITHIN FIVE (5) DAYS OF THE MUTUALLY AGREED UPON SERVICE DATE. IF THE CONDITION IS NOT REMEDIED WITHIN A REASONABLE TIME, THEY ARE INSTRUCTED ON HOW TO CONTACT THE NATIONAL HIGHWAY TRAFFIC SAFETY ADMINISTRATION.

DEFECT INVOLVED

GENERAL MOTORS HAS DECIDED THAT A DEFECT WHICH RELATES TO MOTOR VEHICLE SAFETY EXISTS IN 1997-98 CHEVROLET S-10 TRUCKS WITH ELECTRIC DRIVE. RAPID FOGGING OF THE INTERIOR GLASS CAN OCCUR WITHIN TWO MINUTES AFTER THE HEAT IS TURNED ON IF (1) THE OUTSIDE TEMPERATURE IS BETWEEN 35 AND 76 DEGREES FAHRENHEIT AND (2) WATER HAS COLLECTED ON THE HEAT EXCHANGER DURING PREVIOUS OPERATION OF THE AIR CONDITIONING (WATER CAN REMAIN THERE EVEN SEVERAL DAYS AFTER THE AIR CONDITIONING WAS USED). IF RAPID FOGGING WERE TO OCCUR DURING DRIVING, IT COULD OBSTRUCT THE DRIVER'S VISION AND LEAD TO A CRASH WITHOUT PRIOR WARNING.

ADVISE ALL DRIVERS TO FOLLOW THIS PROCEDURE TO HELP AVOID FOGGING DURING DRIVING:

"STOP AND WAIT" PROCEDURE

NEVER DEPRESS THE HEAT SWITCH WHILE YOU ARE DRIVING. WHEN HEAT IS NEEDED, PARK THE VEHICLE IN A SAFE PLACE. DEPRESS THE HEAT SWITCH. IF NO FOGGING OCCURS AFTER THREE MINUTES, YOU MAY BEGIN DRIVING. IF FOGGING OCCURS, USE THE DEFROST MODE UNTIL THE WINDOWS ARE CLEAR FOR SAFE OPERATION OF THE VEHICLE.

TO REMIND DRIVERS OF THE "STOP AND WAIT" PROCEDURE, WE ARE ENCLOSING A CAUTION LABEL FOR INSTALLATION ON YOUR VEHICLE AND A SUPPLEMENTAL INSERT FOR YOUR OWNER'S MANUAL. YOU SHOULD INSTALL THE ENCLOSED CAUTION LABEL ON YOUR VEHICLE ACCORDING TO THE ATTACHED INSTRUCTIONS OR YOUR CHEVROLET DEALER WILL INSTALL IT FOR YOU AT NO CHARGE.

USE OF AN "ANTI-FOGGING" AGENT ON THE INSIDE SURFACES OF THE VEHICLE'S GLASS, ACCORDING TO THE MANUFACTURER'S DIRECTIONS, CAN REDUCE THE SEVERITY OF FOGGING. THE EFFECTIVENESS OF THESE AGENTS IS A FUNCTION OF MANY VARIABLES, SUCH AS TIME SINCE THE LAST APPLICATION, ANY CLEANING OF THE INSIDE GLASS SURFACES DURING VEHICLE WASH, ETC. ALL DRIVERS SHOULD CONTINUE TO FOLLOW THE PROCEDURES DESCRIBED ABOVE EVEN WHEN AN "ANTI-FOGGING" AGENT IS USED.

VEHICLES INVOLVED

INVOLVED ARE CERTAIN 1997-1998 CHEVROLET S10 ELECTRIC MODEL VEHICLES EQUIPPED WITH AIR CONDITIONING AND BUILT WITHIN THE FOLLOWING VIN BREAKPOINTS:

YEAR DIVISION MODEL PLANT CODE FROM THROUGH

1997 CHEVROLET S-10 SHREVEPORT "8" V8154723 V8208886

1998 CHEVROLET S-10 SHREVEPORT "8" W8100399 W8138496

#### NOTICE: DEALERS SHOULD CONFIRM VEHICLE ELIGIBILITY THROUGH VISS (VEHICLE INFORMATION SERVICE SYSTEM) PRIOR TO BEGINNING CAMPAIGN REPAIRS. [cent ]NOT ALL VEHICLES WITHIN THE ABOVE BREAKPOINTS MAY BE INVOLVED|

INVOLVED VEHICLES HAVE BEEN IDENTIFIED BY VEHICLE IDENTIFICATION NUMBER. COMPUTER LISTINGS CONTAINING THE COMPLETE VEHICLE IDENTIFICATION NUMBER, CUSTOMER NAME AND ADDRESS DATA HAVE BEEN PREPARED, AND ARE BEING FURNISHED TO INVOLVED DEALERS WITH THE CAMPAIGN BULLETIN. THE CUSTOMER NAME AND ADDRESS DATA FURNISHED WILL ENABLE DEALERS TO FOLLOW-UP WITH CUSTOMERS INVOLVED IN THIS CAMPAIGN. ANY DEALER NOT RECEIVING A COMPUTER LISTING WITH THE CAMPAIGN BULLETIN HAS NO INVOLVED VEHICLES CURRENTLY ASSIGNED.

THESE DEALER LISTINGS MAY CONTAIN CUSTOMER NAMES AND ADDRESSES OBTAINED FROM STATE MOTOR VEHICLE REGISTRATION RECORDS. THE USE OF SUCH MOTOR VEHICLE REGISTRATION DATA FOR ANY OTHER PURPOSE IS A VIOLATION OF LAW IN SEVERAL STATES. ACCORDINGLY, YOU ARE URGED TO LIMIT THE USE OF THIS LISTING TO THE FOLLOW-UP NECESSARY TO COMPLETE THIS CAMPAIGN.

PARTS INFORMATION

PARTS REQUIRED TO COMPLETE THIS CAMPAIGN WERE INDIVIDUALLY SENT TO OWNERS OF RECORD. ADDITIONAL PARTS MAY BE OBTAINED FROM CHEVROLET SERVICE.

PART NUMBER DESCRIPTION QUANTITY/ VEHICLE

15035926 OWNER'S MANUAL SUPPLEMENT 1

27004661 LABEL 1

CUSTOMER NOTIFICATION

CUSTOMERS WILL BE NOTIFIED OF THIS CAMPAIGN ON THEIR VEHICLES BY GENERAL MOTORS (SEE COPY OF TYPICAL CUSTOMER LETTER INCLUDED WITH THIS BULLETIN - ACTUAL DIVISIONAL LETTER MAY VARY SLIGHTLY).

DEALER CAMPAIGN RESPONSIBILITY

ALL UNSOLD NEW VEHICLES IN DEALERS' POSSESSION AND SUBJECT TO THIS CAMPAIGN MUST BE HELD AND INSPECTED/REPAIRED PER THE SERVICE PROCEDURE OF THIS CAMPAIGN BULLETIN BEFORE CUSTOMERS TAKE POSSESSION OF THESE VEHICLES.

DEALERS ARE TO SERVICE ALL VEHICLES SUBJECT TO THIS CAMPAIGN AT NO CHARGE TO CUSTOMERS, REGARDLESS OF MILEAGE, AGE OF VEHICLE, OR OWNERSHIP, FROM THIS TIME FORWARD.

CUSTOMERS WHO HAVE RECENTLY PURCHASED VEHICLES SOLD FROM YOUR VEHICLE INVENTORY, AND FOR WHICH THERE IS NO CUSTOMER INFORMATION INDICATED ON THE DEALER LISTING, ARE TO BE CONTACTED BY THE DEALER. ARRANGEMENTS ARE TO BE MADE TO MAKE THE REQUIRED CORRECTION ACCORDING TO THE INSTRUCTIONS CONTAINED IN THIS BULLETIN. THIS COULD BE DONE BY MAILING TO SUCH CUSTOMERS A COPY OF THE APPROPRIATE DIVISIONAL CUSTOMER LETTER ACCOMPANYING THIS BULLETIN. CAMPAIGN FOLLOW-UP CARDS SHOULD NOT BE USED FOR THIS PURPOSE, SINCE THE CUSTOMER MAY NOT AS YET HAVE RECEIVED THE NOTIFICATION LETTER.

IN SUMMARY, WHENEVER A VEHICLE SUBJECT TO THIS CAMPAIGN ENTERS YOUR VEHICLE INVENTORY, OR IS IN YOUR DEALERSHIP FOR SERVICE IN THE FUTURE, PLEASE TAKE THE STEPS NECESSARY TO BE SURE THE CAMPAIGN CORRECTION HAS BEEN MADE BEFORE SELLING OR RELEASING THE VEHICLE.

SERVICE PROCEDURE

1. ENSURE MOUNTING SURFACE IS CLEAN.

2. INSTALL CAUTION LABEL ON HEADLINER CENTERED BETWEEN VISORS (SEE FIGURE).

3. INSERT THE SUPPLEMENT IN THE OWNER'S MANUAL.

4. INSTALL THE GM CAMPAIGN IDENTIFICATION LABEL.

CAMPAIGN IDENTIFICATION LABEL

EACH VEHICLE CORRECTED IN ACCORDANCE WITH THE INSTRUCTIONS OUTLINED IN THIS PRODUCT CAMPAIGN BULLETIN WILL REQUIRE A "CAMPAIGN IDENTIFICATION LABEL". EACH LABEL PROVIDES A SPACE TO INCLUDE THE CAMPAIGN NUMBER AND THE FIVE (5) DIGIT DEALER CODE OF THE DEALER PERFORMING THE CAMPAIGN SERVICE. THIS INFORMATION MAY BE INSERTED WITH A TYPEWRITER OR A BALL POINT PEN.

EACH "CAMPAIGN IDENTIFICATION LABEL" IS TO BE LOCATED ON THE RADIATOR CORE SUPPORT IN AN AREA WHICH WILL BE VISIBLE WHEN THE VEHICLE IS BROUGHT IN BY THE CUSTOMER FOR PERIODIC SERVICING. WHEN INSTALLING THE CAMPAIGN IDENTIFICATION LABEL, BE SURE TO PULL THE TAB TO ALLOW ADHESION OF THE CLEAR PROTECTIVE COVERING. ADDITIONAL CAMPAIGN IDENTIFICATION LABELS CAN BE OBTAINED FROM VISPAC INCORPORATED BY CALLING 1-800-269-5100 (MONDAY-FRIDAY, 8:00 A.M. TO 4:30 P.M. EST). ASK FOR ITEM NUMBER S-1015 WHEN ORDERING.

APPLY THE "CAMPAIGN IDENTIFICATION LABEL" ONLY ON A CLEAN, DRY SURFACE.

CLAIM INFORMATION

SUBMIT A PRODUCT CAMPAIGN CLAIM WITH THE INFORMATION INDICATED BELOW:

PART FAILED PARTS LABOR LABOR NET REPAIR PERFORMED COUNT PART NO. ALLOW CC-FC OP * HOURS ITEM

INSERT SUPPLEMENT AND INSTALL LABEL. ** N/A N/A MA-96 V0187 0.2

* FOR CAMPAIGN ADMINISTRATIVE ALLOWANCE, ADD 0.1 HOURS TO THE "LABOR HOURS".

REFER TO THE GENERAL MOTORS CORPORATION CLAIMS PROCESSING MANUAL FOR DETAILS ON PRODUCT CAMPAIGN CLAIM SUBMISSION.

FIGURES: 1

GM BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THESE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE TOOLS, EQUIPMENT, SAFETY INSTRUCTIONS, AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

WE SUPPORT VOLUNTARY TECHNICIAN CERTIFICATION

CENTRAL OFFICE CHEVROLET MOTOR DIVISION GENERAL MOTORS CORPORATION 100 RENAISSANCE CENTER, P.O. BOX 100, DETROIT, MI 48265-1000

C98031-S

AUGUST, 1998

DEAR S-10 ELECTRIC OWNER:

THIS NOTICE IS SENT TO YOU IN ACCORDANCE WITH THE NATIONAL TRAFFIC AND MOTOR VEHICLE SAFETY ACT.

REASON FOR THIS RECALL:

GENERAL MOTORS HAS DECIDED THAT A DEFECT WHICH RELATES TO MOTOR VEHICLE SAFETY EXISTS IN 1997 AND 1998 CHEVROLET S-10 TRUCKS WITH ELECTRIC DRIVE. RAPID FOGGING OF THE INTERIOR GLASS CAN OCCUR WITHIN TWO MINUTES AFTER THE HEAT IS TURNED ON IF (1) THE OUTSIDE TEMPERATURE IS BETWEEN 35 AND 76 DEGREES FAHRENHEIT AND (2) WATER HAS COLLECTED ON THE HEAT EXCHANGER DURING PREVIOUS OPERATION OF THE AIR CONDITIONING (WATER CAN REMAIN THERE EVEN SEVERAL DAYS AFTER THE AIR CONDITIONING WAS USED). IF RAPID FOGGING WERE TO OCCUR DURING DRIVING, IT COULD OBSTRUCT THE DRIVER'S VISION AND LEAD TO A CRASH WITHOUT PRIOR WARNING.

WHAT YOU SHOULD DO: ADVISE ALL DRIVERS TO FOLLOW THIS PROCEDURE TO HELP AVOID FOGGING DURING DRIVING:

"STOP AND WAIT" PROCEDURE

NEVER DEPRESS THE HEAT SWITCH WHILE YOU ARE DRIVING. WHEN HEAT IS NEEDED, PARK THE VEHICLE IN A SAFE PLACE. DEPRESS THE HEAT SWITCH. IF NO FOGGING OCCURS AFTER THREE MINUTES, YOU MAY BEGIN DRIVING. IF FOGGING OCCURS, USE THE DEFROST MODE UNTIL THE WINDOWS ARE CLEAR FOR SAFE OPERATION OF THE VEHICLE.

USE OF AN "ANTI-FOGGING" AGENT ON THE INSIDE SURFACES OF THE VEHICLE'S GLASS, ACCORDING TO THE MANUFACTURER'S DIRECTIONS, CAN REDUCE THE SEVERITY OF FOGGING. THE EFFECTIVENESS OF THESE AGENTS IS A FUNCTION OF MANY VARIABLES, SUCH AS TIME SINCE THE LAST APPLICATION, ANY CLEANING OF THE INSIDE GLASS SURFACES DURING VEHICLE WASH, ETC. ALL DRIVERS SHOULD CONTINUE TO FOLLOW THE PROCEDURES DESCRIBED ABOVE EVEN WHEN AN "ANTI-FOGGING" AGENT IS USED.

WHAT WE WILL DO: TO REMIND DRIVERS OF THE "STOP AND WAIT" PROCEDURE, WE ARE ENCLOSING A CAUTION LABEL FOR INSTALLATION ON YOUR VEHICLE AND A SUPPLEMENTAL INSERT FOR YOUR OWNER'S MANUAL. YOU SHOULD INSTALL THE ENCLOSED CAUTION LABEL ON YOUR VEHICLE ACCORDING TO THE ATTACHED INSTRUCTIONS OR YOUR CHEVROLET DEALER WILL INSTALL IT FOR YOU AT NO CHARGE.

HOW LONG WILL THE REPAIR TAKE? THE LENGTH OF TIME REQUIRED FOR THE DEALER TO PERFORM THIS INSPECTION AND SERVICE CORRECTION, IF REQUIRED, IS APPROXIMATELY 10-15 MINUTES. ADDITIONAL TIME MAY BE REQUIRED TO SCHEDULE AND PROCESS YOUR VEHICLE. IF YOUR DEALER HAS A LARGE NUMBER OF VEHICLES AWAITING SERVICE, THIS ADDITIONAL TIME MAY BE SIGNIFICANT. PLEASE ASK YOUR DEALER IF YOU WISH TO KNOW HOW MUCH ADDITIONAL TIME WILL BE NEEDED.

IF, AFTER CONTACTING YOUR CHEVROLET DEALER, YOU ARE STILL NOT SATISFIED WE HAVE DONE OUR BEST TO REMEDY THIS CONDITION WITHOUT CHARGE AND WITHIN A REASONABLE TIME, YOU MAY WISH TO WRITE THE ADMINISTRATOR, NATIONAL HIGHWAY TRAFFIC SAFETY ADMINISTRATION, 400 SEVENTH ST., S.W., WASHINGTON, DC 20590 , OR CALL 1-800- 424-9393 (WASHINGTON, DC RESIDENTS USE [cent ]202|366-0123).

GENERAL MOTORS PLACES THE HIGHEST PRIORITY ON OWNER SAFETY AND SATISFACTION. WE SINCERELY REGRET ANY INCONVENIENCE THIS MAY HAVE CAUSED YOU.

CHEVROLET MOTOR DIVISION GENERAL MOTORS CORPORATION

ENCLOSURE

#### CAUTION

LABEL INSTALLATION PROCEDURE

1. ENSURE MOUNTING SURFACE IS CLEAN.

2. INSTALL CAUTION LABEL ON HEADLINER CENTERED BETWEEN VISORS AS SHOWN IN FIGURE 1 BELOW.

FIGURE 1 - CAUTION LABEL INSTALLATION

SUPPLEMENTAL INSERT INSTALLATION PROCEDURE

1. INSERT THE SUPPLEMENT IN THE OWNER'S MANUAL

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.