Park/Neutral Position and Backup Lamp Switch Adjustment. Chevrolet Brazil Blazer 1997

For 1990-2009 cars

• | Check the switch for proper operation.

• | The engine must be in the P (Park) or N (Neutral) positions only. If adjustment is required, loosen the switch retaining bolts and rotate the switch slightly.

• | Tighten the bolts and check the switch for proper operation.

• | Repeat the switch adjustment procedure until the engine starts when the shift lever is positioned in park and neutral.