ENGINE ROUGH, MISS & OXYGEN SENSOR DTCS. Chevrolet Brazil Blazer 1997

For 1990-2009 cars

# ENGINE ROUGH, MISS & OXYGEN SENSOR DTCS

#### SUBJECT: ENGINE ROUGH, MISS, AND OXYGEN SENSOR DTCS (REPLACE OXYGEN SENSOR JUMPER HARNESS)

#### MODELS: 1996-97 CHEVROLET AND GMC S/T TRUCKS 1996-97 OLDSMOBILE BRAVADA 1997 ISUZU WITH 4.3L V6 ENGINES (VINS W, X - RPOS L35, LF6)

#### CONDITION:

SOME OWNERS MAY COMMENT ABOUT AN ENGINE MISS AND/OR ROUGHNESS AND A SES LIGHT.

#### CAUSE:

SOME OXYGEN SENSORS ON THE PASSENGER SIDE OF THE VEHICLE HAVE BEEN FOUND TO BE DAMAGED DUE TO WATER INTRUSION. APPROXIMATELY 20% OF THE OXYGEN SENSORS RETURNED FOR ANALYSIS ON THESE MODELS HAVE EXHIBITED THIS CONDITION. IF ANY OXYGEN SENSOR RELATED DTC IS STORED, MOISTURE MAY HAVE ENTERED THE JUMPER HARNESS THAT CONNECTS THE THREE PASSENGER SIDE OXYGEN SENSORS TO THE MAIN ENGINE HARNESS AND DAMAGE THE SENSOR AND THE HARNESS. OXYGEN SENSORS THAT HAVE BEEN DAMAGED BY WATER WILL HAVE CORROSION ON ONE OR MORE OF THE SENSORS (4) TERMINALS. THE JUMPER HARNESS CONNECTOR AT THE SAME LOCATION MAY OR MAY NOT SHOW SIMILAR CORROSION. IF THERE IS UNDETECTED MOISTURE IN THE JUMPER HARNESS, A REPLACEMENT OXYGEN SENSOR CAN BE DAMAGED RESULTING IN A REPEAT FAILURE. IN ADDITION, A REPLACEMENT OXYGEN SENSOR MAY BE MISDIAGNOSED AS FAULTY WHEN THE ACTUAL FAULT IS UNDETECTED MOISTURE IN THE JUMPER HARNESS.

#### CORRECTION:

1. FOLLOW THE STRATEGY BASED DIAGNOSTICS AND PUBLISHED PROCEDURES FOR THE SPECIFIC SYMPTOM AND DTC. 2. INSPECT THE OXYGEN SENSOR CONNECTORS FOR SIGNS OF MOISTURE OR "BLUISH-GREEN" CORROSION ON THE CONTACTS AND IN THE CONNECTOR CAVITIES. 3. IF WATER INTRUSION IS SUSPECTED, BUT NO CORROSION IS EVIDENT, SENSOR FUNCTION MAY BE CHECKED USING A DVOM TO MEASURE RESISTANCE ACROSS THE SENSOR'S PURPLE AND TAN CONTACTS. A DEFECTIVE SENSOR WILL SHOW A RESISTANCE VALUE. A GOOD SENSOR WILL SHOW NO CONTINUITY (INFINITE RESISTANCE) OR "OPEN". 4. IF THESE SIGNS ARE DETECTED, REPLACE THE OXYGEN SENSOR JUMPER HARNESS AND ALL AFFECTED OXYGEN SENSOR(S). DO NOT ATTEMPT TO REPAIR THE JUMPER HARNESS BY CLEANING OR REPLACEMENT OF CORRODED TERMINALS. DO NOT USE OR APPLY ANY TYPE OF SEALANT ANYWHERE IN THE OXYGEN SENSOR CONNECTORS OR WIRES. REPAIR ATTEMPTS TO OXYGEN SENSOR HARNESSES GENERALLY RESULT IN A REPEAT FAILURE. 5. RECORD ALL DTCS ENCOUNTERED DURING PROBLEM DIAGNOSIS ON THE REPAIR ORDER. THIS IS NEEDED FOR ENGINEERING ANALYSIS OF THE COMPONENTS. 6. VERIFY THE SYMPTOM AND/OR DTC IS CORRECTED BEFORE RETURNING THE VEHICLE TO THE OWNER.

#### IMPORTANT

THE NEW JUMPER HARNESS MUST BE ROUTED ACCORDING TO THE COMPONENT LOCATION VIEWS IN SECTION 8A OF THE APPROPRIATE S/T TRUCK SERVICE MANUAL.

PARTS INFORMATION

PART NUMBER DESCRIPTION QUANTITY 12173753 OXYGEN SENSOR WIRING HARNESS, 2WD 1 12173754 OXYGEN SENSOR WIRING HARNESS, 4WD 1

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

WARRANTY INFORMATION FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION DESCRIPTION LABOR TIME N6271 JUMPER HARNESS, REPLACE .5 HR.

#### IMPORTANT: LABOR OPERATION IS CODED TO BASE VEHICLE COVERAGE IN THE WARRANTY SYSTEM.

FIGURES: 0 ATTACHMENTS: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997. GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.