For 1990-2009 cars

### Inspection Procedure

• | Check the pinion gear shaft for unusual wear.

• | Check the pinion and the side gear teeth for wear, cracks, scoring and spalling.

• | Check the thrust washers for wear.

• | Check the fit of the side gears in the differential case and on the axle shafts.

• | Check the differential case for cracks and scoring and replace all of the worn parts as necessary.