For 1990-2009 cars

### Removal Procedure

1. Apply the parking brake.
2. Block the wheels.
3. Drain all the reservoirs. Refer to Draining Reservoirs .
4. Disconnect the air lines at the valve. Refer to Hose and Line Replacement - Nylon and Metal Compression .
5. Remove the mounting bolts (6).
6. Remove the washers (3).
7. Remove the nuts (2).
8. Remove the front axle limiting (ratio) valve (4).

### Installation Procedure

1. Install the front axle limiting (ratio) valve (4).
2. Install the bolts (6).
3. Install the washers (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the nuts (2).

Tighten
Tighten the front axle limiting, ratio valve nuts (2) to 22 N·m (16 lb ft).

5. Connect the air lines. Refer to Hose and Line Replacement - Nylon and Metal Compression .
6. Start the engine.
7. Charge the system air pressure to the governor cut-out point.
8. Stop the engine.
9. Check for air leaks using a soap solution.
10. Check for proper operation.
11. Remove the wheel blocks.