For 1990-2009 cars

#### Tools Required

J 36850 Transjel® Lubricant

1. Install the vehicle speed sensor O-ring (3) onto the turbine speed sensor (2).
2. Apply J 36850 to the O-ring (3).
3. Install the turbine speed sensor (2) into the transmission case.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the vehicle speed sensor bolt (1) into the transmission case.

Tighten
Tighten the bolt to 12 N·m (108 lb in).