For 1990-2009 cars

Application | Specification
--- | ---
Inspect | Set
Angular Toe-In per Wheel-Loaded | 0.028-0.056 degrees | 0.028 degrees
Camber-Unloaded-All except 16k Axle | 0.50-1.00 degrees | Non-adjustable
Camber-Loaded-With 16k Axle | LH 0.75 degrees RH 0.25 degrees | Non-adjustable
Caster-Loaded-All except 16k Axle | 3.0-5.0 degrees | Non-adjustable
King Pin Inclination-All except 16k Axle | 6 degrees | Non-adjustable
King Pin Inclination-With 16k Axle | LH 5.25 degrees RH 5.75 degrees | Non-adjustable
Linear Sum Toe-In-Loaded | 0.7940-1.5875 mm (0.03125-0.0625 in) | 0.7940 mm (-0.03125 in)
Loaded: It is preferable that the vehicle be at normal operating load during alignment checks and resets. Unloaded: It is preferred that the vehicle be at curb operating load during alignment checks and resets.