For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Lining Replacement Thickness | 1.60 mm | 0.063 in
Brake Lining to Brake Rotor Maximum Clearance | 0.13 mm | 0.005 in
Brake Rotor OD Runout | 0.76 mm | 0.030 in
Brake Rotor Thickness Variation | 0.05 mm | 0.002 in
Brake Rotor Total Indicated Runout (TIR) | 0.13 mm | 0.005 in
Front Hub and Bearing Assembly Lateral Runout | 0.040 mm | 0.0016 in