For 1990-2009 cars

## Transverse Rod Replacement With GPG

### Removal Procedure

1. Remove the locknuts (4) and the washers (3) that connect the transverse rod (1) to the frame.
2. Remove the locknuts (4) and the washers (3) that fasten the transverse rod (1) to the axle housing (2).
3. Remove the transverse rod (1).
4. Remove the transverse rod bracket from the frame.
5. Inspect the transverse rod bushings. If the transverse rod bushings are worn or damaged, remove the bushing from the transverse rod (1).

### Installation Procedure

1. Install the bushings in the transverse rod.
2. Position the transverse rod (1) in the bracket on the axle housing (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the following components:

• | The transverse rod bolt (7)

• | The washers (6)

• | The locknuts (4) that fasten the rod to the bracket

Tighten
Tighten the locknut to 508 N·m (375 lb ft) for models with GPG.

4. Install the following components:

• | The reinforcement bolts

• | The washers

• | The locknuts that fasten the torque rod and the bracket to the frame

Tighten
Tighten the rod bar pin nuts to 298 N·m (220 lb ft).

## Transverse Rod Replacement Except GPG

### Removal Procedure

1. Remove the locknuts (4) and the washers (3) that connect the transverse rod (1) to the frame.
2. Remove the locknuts (6) and the washers (2, 5) that fasten the transverse rod (4) to the axle housing (3).
3. Remove the transverse rod (4).
4. Remove the transverse rod bracket from the frame.
5. Inspect the transverse rod bushings. If the transverse rod bushings are worn or damaged, remove the bushing from the transverse rod (1).

### Installation Procedure

1. Install the bushings in the transverse rod.
2. Position the transverse rod (4) in the bracket on the axle housing (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the following components:

• | Transverse rod bolts (1)

• | The washers (2)

• | The locknuts (6) that fasten the rod to the bracket

Tighten
Tighten the locknut on the transverse rod taper pin to 298 N·m (220 lb ft) for models without GPG.

4. Install the following components:

• | The reinforcement bolts (7)

• | The washers (6, 3)

• | The locknuts (4)

Tighten
Tighten the pin nuts on the transverse rod bar to 298 N·m (220 lb ft).