For 1990-2009 cars

### Removal Procedure

1. Apply the parking brake.
2. Block the vehicle wheels.
3. Loosen the spring clip from the unhinged side of the mounting baffle.
4. Remove the air compressor air filter strainer cover.
5. Open the air compressor air strainer filter cover.
6. Remove the air compressor air strainer filter.

### Installation Procedure

1. Install the new air compressor air strainer filter.
2. Install the air compressor air strainer filter cover.
3. Secure the air compressor air strainer filter cover with the spring clip.
4. Remove the wheel blocks.