For 1990-2009 cars

Important: DO NOT replace the retaining ring in the low and reverse clutch housing unless:

• | The retaining ring is damaged.

• | The low and reverse clutch housing is to be replaced.

1. Position the low and reverse clutch housing (2) on the worktable so that the inside of the cover is facing down.
2. Remove retaining ring (1).
3. Install a new retaining ring (1).
4. Make sure the retaining ring is seated.