For 1990-2009 cars

### Circuit Description

The throttle actuator control (TAC) module contains data which is essential for proper TAC system operation. The TAC module continuously tests the integrity of this data. When the TAC module is unable to write or read data to and from RAM or the TAC module is unable to correctly read data from the flash memory or an internal TAC module processor fault is detected, this diagnostic trouble code (DTC) sets.

### Conditions for Running the DTC

• | DTC P1518 is not set.

• | The ignition switch is in the crank or run position.

• | The ignition voltage is greater than 6 volts.

### Conditions for Setting the DTC

• | The TAC module determines that an internal data test did not pass.

• | All above conditions are met for less than 1 second.

### Action Taken When the DTC Sets

• | The control module illuminates the malfunction indicator lamp (MIL) when the diagnostic runs and fails.

• | The control module records the operating conditions at the time the diagnostic fails. The control module stores this information in the Freeze Frame and/or the Failure Records.

• | The control module commands the TAC system to operate in the Reduced Engine Power mode.

• | A message center or an indicator displays Reduced Engine Power.

• | Under certain conditions the control module commands the engine OFF.

### Conditions for Clearing the MIL/DTC

• | The control module turns OFF the malfunction indicator lamp (MIL) after 3 consecutive ignition cycles that the diagnostic runs and does not fail.

• | A current DTC, Last Test Failed, clears when the diagnostic runs and passes.

• | A history DTC clears after 40 consecutive warm-up cycles, if no failures are reported by this or any other emission related diagnostic.

• | Clear the MIL and the DTC with a scan tool.

### Diagnostic Aids

• | Ensure that the starting and charging systems are operating properly. Low system voltage can cause this DTC to set.

• | Inspect the TAC module connectors for signs of water intrusion. When this occurs, multiple DTCs could be set with no circuit or component conditions found during diagnostic testing.

• | When the TAC module detects a condition within the TAC system, more than one TAC system related DTC may set. This is due to the many redundant tests run continuously on this system. Locating and repairing one individual condition may correct more than one DTC. Disconnecting components during testing may set additional DTCs. Keep this in mind when reviewing the stored information, Capture Info.

### Test Description

The number below refers to the step number on the diagnostic table.

1. When the TAC module detects a condition within the TAC system, more than one TAC system related DTC may set. This is due to the many redundant tests run continuously on this system. Locating and repairing one individual condition may correct more than one DTC. Disconnecting components during testing may set additional DTCs. Keep this in mind when reviewing the stored information, Capture Info.

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Diagnostic System Check-Engine Controls? | Go to Step 2 | Go to Diagnostic System Check - Engine Controls
2 | Replace the TAC module. Refer to Electronic Throttle Actuator Control Module Replacement . Did you complete the replacement? | Go to Step 3 | --
3 |

1. Use the scan tool in order to clear the DTCs.
2. Turn OFF the ignition for 30 seconds.
3. Start the engine.
4. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text.

Does the DTC run and pass?

Go to Step 4

Go to Step 2

4 | With a scan tool, observe the stored information, Capture Info. Does the scan tool display any DTCs that you have not diagnosed? | Go to Diagnostic Trouble Code (DTC) List | System OK