For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column - Standard Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Steering Wheel and Column
2 | Verify that a high shift effort is required in order to shift out of the PARK position. Does the shifter operate normally? | System OK | Go to Step 3
3 | Inspect for worn or damaged shift linkage components. Are the shift linkage components worn or damaged? | Go to Step 5 | Go to Step 4
4 | Inspect the shift cable for binding or misadjustment. Is the shift cable binding or misadjusted? | Go to Step 6 | Go to Step 5
5 | Replace the shift linkage. Did you complete the repair? | Go to Step 7 | --
6 | Adjust the shift cable. Did you complete the repair? | Go to Step 7 | --
7 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2