For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Battery Inspection/Test? | Go to Step 2 | Go to Battery Inspection/Test
2 | Turn ON the ignition, with the engine OFF observe the charge indicator on the instrument cluster (IPC). Is the charge indicator illuminated? | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems | Go to Step 3
3 | Replace the charge indicator lamp in the instrument cluster. Refer to Instrument Cluster Replacement in Instrument Panel, Gages and Console. Did you complete the replacement? | Go to Step 4 | --
4 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2