For 1990-2009 cars

#### Tools Required

• | J 43778 1-2-3-4, 4-5 Clutch Bushing Installer

• | J 8092 Universal Driver

### Removal Procedure

Important: DO NOT score the 1-2-3-4, 4-5 clutch housing bore when removing the clutch housing bushing.

1. Gently tap the bushing through the inside of the 1-2-3-4, 4-5 clutch housing until the bushing becomes dislodged.
2. Remove the bushing (2) from the 1-2-3-4, 4-5 clutch housing (1).
3. Remove any nicks or burrs with a crocus cloth.

### Installation Procedure

1. Position the 1-2-3-4, 4-5 clutch housing (4) on a press so that the front of the housing is facing up.

Important: The preferred method for installing the 1-2-3-4, 4-5 clutch housing bushing is to use the J 43778 and a press. If a press is not available, use the J 43778 and the J 8092 .

2. If the bushing will be installed without a press, install the large end of J 43778 (2) onto J 8092 (1).
3. Install a new bushing (3) onto J 43778 (2).
4. Using J 8092 , press or drive the new bushing into the clutch housing.

Specification
The bushing depth measurement is flush to 0.25 mm (0.01 in) below the 1-2-3-4, 4-5 clutch housing surface.