For 1990-2009 cars

Important: Do not replace missing balance weights or straighten a bent tube.

An unbalanced propeller shaft and universal joint assembly may be caused by one or more of the following conditions:

• | Missing balance weights

• | Bent, dented, or damaged tubing

• | Worn slip spline (inboard type)

• | Foreign material on the propeller shaft tubing or the end yokes

• | Improperly installed propeller shaft and universal joint assembly