For 1990-2009 cars

Table 1: | Cigar Lighter
Table 2: | Fuse Block 1 -- Underhood
Table 3: | Fuse Block 2 -- Underhood
Table 4: | Ignition Switch C1
Table 5: | Ignition Switch C2
Table 6: | Upfitter Accessory Feed Connector
Table 7: | Upfitter AUX WRG Connector, Exterior
Table 8: | Upfitter AUX WRG Connector, Interior

#### Cigar Lighter

Connector Part Information |

• | 12047699

• | 2 Way M Miscellaneous Family Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 240 | Battery Positive Voltage
B | BLK | 250 | Ground

### Convenience Center

Connector Part Information |

• | 12084698

• | Convenience Center

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-K | -- | -- | Not Used
L1 | ORN | 1640 | Battery Positive Voltage
L2 | BRN | 441 | Ignition 3 Voltage
L3 | -- | -- | Not Used
L4 | BRN | 1041 | Ignition 3 Voltage
L5 | BLK | 250 | Ground
M1 | TAN | 12 | Headlamp Low Beam Supply Voltage
M2 | PNK | 39 | Ignition 1 Voltage
M3 | PPL | 544 | DRL Relay Contact-Normally Closed
M4 | WHT | 815 | DRL Diode Signal
M5 | LT GRN /BLK | 592 | DRL Relay Control
N1 | GRY | 120 | Fuel Pump Supply Voltage (L18)
N1 | ORN | 740 | Battery Positive Voltage (LG5)
N2 | DK GRN /WHT | 465 | Fuel Pump Relay Control (L18)
N2 | BRN | 441 | Ignition 3 Voltage (LG5)
N3 | ORN | 490 | Fuel Pump Prime Supply Voltage (L18)
N3 | -- | -- | Not Used (LG5)
N4 | ORN | 40 | Battery Positive Voltage (L18)
N4 | BRN | 841 | Ignition 3 Voltage (LG5)
N5 | BLK/WHT | 451 | Ground (L18)
N5 | BLK | 250 | Ground (LG5)
P1 | ORN | 1340 | Battery Positive Voltage
P2 | YEL | 143 | Accessory Voltage
P3 | -- | -- | Not Used
P4 | YEL | 43 | Accessory Voltage
P5 | BLK | 250 | Ground
R1 | ORN | 440 | Battery Positive Voltage
R2 | BRN | 441 | Ignition 3 Voltage
R3 | YEL | 1649 | Blower Enable Relay Contact-Normally Closed
R4 | LT BLU | 188 | Blower Enable Relay Contact-Normally Open
R5 | BRN | 247 | Blower Enable Relay Control
S1 | PPL | 65 | Blower Motor Supply Voltage
S2 | BRN | 441 | Ignition 3 Voltage
S3 | TAN | 63 | Medium 1 Blower Motor Control
S4 | YEL | 1649 | Blower Enable Relay Contact-Normally Closed
S5 | ORN | 52 | High Blower Control
T1 | ORN | 1140 | Battery Positive Voltage-Super Chassis with JE3 and J71
T1 | ORN | 840 | Battery Positive Voltage-Super Chassis with JE5 and RQ3/U86
T2 | PNK | 39 | Ignition 1 Voltage-Super Chassis with JE3 and J71
T2 | DK GRN | 21 | Roof Clearance Lamp Switch Signal-Super Chassis with JE5 and RQ3/U86
T3 | -- | -- | Not Used
T4 | YEL | 1492 | Park Brake Switch Supply Voltage-Super Chassis with JE3 and J71
T4 | DK BLU | 45 | Park Lamp Supply Voltage-Super Chassis with JE5 and RQ3/U86
T5 | PNK/BLK | 1929 | Park Brake Pump Motor Relay Control-Super Chassis with JE3 and J71
T5 | BLK | 250 | Ground- Super Chassis with JE5 and RQ3/U86
U1 | ORN | 340 | Battery Positive Voltage
U2 | LT BLU | 13 | Headlamp Switch Park Lamps Signal
U3 | -- | -- | Not Used
U4 | BRN | 9 | Park Lamp Supply Voltage
U5 | BLK | 250 | Ground
V1 | RED | 442 | Battery Positive Voltage
V2 | BRN | 441 | Ignition 3 Voltage
V3 | -- | -- | Not Used
V4 | BRN | 41 | Ignition 3 Voltage
V5 | BLK | 250 | Ground
W1 | -- | -- | Not Used-Early LG5
W1 | ORN | 2140 | Battery Positive Voltage-All Others
W2 | -- | -- | Not Used-Early LG5
W2 | BRN | 441 | Ignition 3 Voltage-All Others
W3 | -- | -- | Not Used
W4 | -- | -- | Not Used-Early LG5
W4 | PPL | 638 | Power Window Relay-Normally Open Contact-All Others
W5 | -- | -- | Not Used-Early LG5
W5 | BLK | 250 | Ground-All Others
X1-X2 | ORN | 140 | Battery Positive Voltage
X3 | -- | -- | Not Used
X4 | DK GRN | 29 | Horn Control
X5 | TAN | 28 | Horn Relay Control

#### Fuse Block -- I/P -- Rear View

(1) | Fuse Block -- I/P (L18)
(2) | Fuse Block -- I/P (LG5)

Connector Part Information |

• | 15359179 (L18)

• | 15355292 (Early LG5)

• | 15359180 (Late LG5)

• | Fuse Block - I/P (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | PNK | 139 | Ignition 1 Voltage (L18)
A1 | ORN | 2040 | Battery Positive Voltage-Early LG5 with Super Chassis
A1 | PPL | 2000 | Battery Positive Voltage-Late LG5 with MTW/MX4
A2 | PNK | 239 | Ignition 1 Voltage-L18
A2 | ORN | 2140 | Battery Positive Voltage-Early LG5 with Super Chassis
A2 | ORN | 40 | Battery Positive Voltage-Late LG5 with MWF/MTW/MX4
A3 | BRN | 241 | Ignition 3 Voltage
A4 | BRN | 341 | Ignition 3 Voltage
A5 | YEL | 143 | Accessory Voltage
B1 | PPL | 2000 | Ignition 1 Relay Output-Normally Open (L18)
B1 | RED | 1342 | Battery Positive Voltage-Early LG5 with Super Chassis
B1 | RED | 42 | Battery Positive Voltage- Late LG5 with MTW/MX4
B2 | -- | -- | Bussed From B1
B3 | -- | -- | Bussed From B4
B4 | BRN | 41 | Ignition 3 Voltage
B5 | BRN | 4 | Accessory Voltage
C1 | ORN | 1340 | Battery Positive Voltage
C2 | ORN | 40 | Battery Positive Voltage-Early LG5 with MWF
C2 | ORN | 2140 | Battery Positive Voltage-All Others with Super Chassis
C3 | ORN | 40 | Battery Positive Voltage (L18)
C3 | ORN | 740 | Battery Positive Voltage -LG5 with Super Chassis
C4 | ORN | 1540 | Battery Positive Voltage
C5 | ORN | 1240 | Battery Positive Voltage
D1 | RED | 642 | Battery Positive Voltage
D2 | RED | 1442 | Battery Positive Voltage-Early LG5 with MWF
D2 | RED | 1342 | Battery Positive Voltage-All Others with Super Chassis
D3 | RED | 42 | Battery Positive Voltage (L18)
D3 | -- | -- | Bussed From D4 (LG5)
D4 | RED | 542 | Battery Positive Voltage
D5 | -- | -- | Bussed From D4
E1 | ORN | 1640 | Battery Positive Voltage
E2 | ORN | 640 | Battery Positive Voltage
E3 | ORN | 1140 | Battery Positive Voltage-Super JE3 with J71
E4 | BRN | 541 | Ignition 3 Voltage
E5 | BRN | 441 | Ignition 3 Voltage
F1 | -- | -- | Bussed From F2
F2 | RED | 1242 | Battery Positive Voltage
F3 | -- | -- | Bussed From F2
F4 | -- | -- | Bussed From F5
F5 | ORN | 300 | Ignition 3 Voltage
G1 | PNK | 39 | Ignition 1 Voltage
G2 | ORN | 240 | Battery Positive Voltage
G3 | ORN | 140 | Battery Positive Voltage
G4 | ORN | 440 | Battery Positive Voltage
G5 | PPL | 2000 | Ignition 1 Relay Output-Normally Open (L18)
G5 | RED | 1542 | Battery Positive Voltage-Early LG5
G5 | RED | 42 | Battery Positive Voltage-Late LG5
H1 | PNK | 3 | Ignition Switch Output-Ignition 1
H2 | -- | -- | Bussed From H3
H3 | RED | 842 | Battery Positive Voltage
H4 | -- | -- | Bussed From H3
H5 | PNK | 339 | Ignition 1 Voltage (L18)
H5 | ORN | 2240 | Battery Positive Voltage (LG5)
J1 | PPL | 806 | Crank Voltage-MWF/MTW/MX4
J1 | GRY | 48 | CPP Switch Signal-All Others
J2 | ORN | 840 | Battery Positive Voltage-Super JE5 with RQ3/U86
J3 | ORN | 340 | Battery Positive Voltage
J4 | ORN | 1040 | Battery Positive Voltage
J5 | ORN | 540 | Battery Positive Voltage (JE3)
K1 | YEL | 5 | Crank Voltage
K2 | -- | -- | Bussed From K3
K3 | RED | 1142 | Battery Positive Voltage
K4 | -- | -- | Bussed From K3
K5 | RED | 342 | Battery Positive Voltage (JE3)

#### Fuse Block -- Underhood -- Bottom View

(1) | Fuse Block 2 -- Underhood
(2) | Fuse Block 1 -- Underhood

#### Fuse Block 1 -- Underhood

Connector Part Information |

• | 12129482

• | Fuse Block 1 - Underhood (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | RED | 342 | Battery Positive Voltage (JE3)
A2 | RED | 142 | Battery Positive Voltage-All Except LG5 with Base Chassis without J71
A3 | RED | 1342 | Battery Positive Voltage-Super Chassis
A4 | RED | 742 | Battery Positive Voltage-Super Chassis with JE3 and J71
A4 | RED | 1442 | Battery Positive Voltage-Super Chassis with JE5 and RQ3/U86
A5 | RED | 842 | Battery Positive Voltage
A6 | RED | 1542 | Battery Positive Voltage-Early LG5
A6 | RED | 42 | Battery Positive Voltage-All Others
B1 | RED | 2 | Battery Positive Voltage (JE3)
B2-B6 | -- | -- | Bussed From B+

#### Fuse Block 2 -- Underhood

Connector Part Information |

• | 12110129

• | Fuse Block 2 - Underhood (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | RED | 542 | Battery Positive Voltage
A2 | RED | 442 | Battery Positive Voltage
A3 | RED | 1142 | Battery Positive Voltage
A4 | RED | 1042 | Battery Positive Voltage
A5 | RED | 1242 | Battery Positive Voltage
A6 | RED | 642 | Battery Positive Voltage
B1-B6 | -- | -- | Bussed From B+

#### Ignition Switch C1

Connector Part Information |

• | 12010966

• | 5 Way F 56 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 5 | Crank Voltage
B | -- | -- | Not Used
C | PNK | 3 | Ignition Switch Output Ignition 1
D | RED | 642 | Battery Positive Voltage
E | BRN | 4 | Accessory Voltage

#### Ignition Switch C2

Connector Part Information |

• | 06294641

• | 4 Way F 56/59 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 300 | Ignition 3 Voltage
B | RED | 442 | Battery Positive Voltage
C | WHT/BLK | 235 | Bulb Test Signal (JE5)
D | LT BLU | 1134 | Park Brake Switch Signal

#### Upfitter Accessory Feed Connector

Connector Part Information |

• | 12015199

• | 2 Way F Metri-Pack 280 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 43 | Accessory Voltage
B | BLK | 250 | Ground

#### Upfitter AUX WRG Connector, Exterior

Connector Part Information |

• | 12065862

• | 4 Way F Metri-Pack 280 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 640 | Battery Positive Voltage
B | BRN | 1041 | Ignition 3 Voltage
C | DK GRN | 909 | To Upfitter AUX WRG Connector, Interior
E | DK BLU | 910 | To Upfitter AUX WRG Connector, Interior

#### Upfitter AUX WRG Connector, Interior

Connector Part Information |

• | 12064752

• | 6 Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 910 | To Upfitter AUX WRG Connector, Exterior
B | DK GRN | 909 | To Upfitter AUX WRG Connector, Exterior
C | BRN | 1041 | Ignition 3 Voltage
D | ORN | 640 | Battery Positive Voltage
E | GRY | 8 | Instrument Panel Lamp Supply Voltage (MWF)
E | -- | -- | Not Used - All Others
F | -- | -- | Not Used