For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 46409 Torque Converter Lifting Handles

Caution: The torque converter dry weight is approximately 29 kg (63 lb). To help avoid personal injury and/or property damage:

• | Use caution when installing, removing, or moving the torque converter.

• | Get help when lifting the torque converter. Assistance from a hoist or another person is required.

• | Make sure J 46409 T-handles are installed securely and that any lifting equipment used can properly support the torque converter.

1. Position the transmission so that the front of the torque converter is facing up.
2. If used, remove 4 bolts and 2 shipping brackets, or remove any other torque converter restraining device.
3. Install 1 J 46409 T-handle into a boss on the front of the torque converter.
4. Install the other J 46409 T-handle into a boss on the front of the torque converter 180 degrees away from the first T-handle.

Caution: Avoid personal injury or property damage when removing or installing the torque converter by seeking an assistant to help lift the torque converter.

5. Remove the torque converter from the converter housing.
6. Place the torque converter on the work table.