For 1990-2009 cars

## Multifunction Turn Signal Lever Replacement On Vehicle

### Removal Procedure

1. Position the windshield wiper switch in the OFF position.
2. Remove the steering column access cover (1) by pulling towards the front of the vehicle.
3. Disconnect the multifunction lever electrical connector (1).
4. Remove the multifunction lever (2).

### Installation Procedure

1. Install the multifunction lever (2).
2. Connect the multifunction lever electrical connector (1).
3. Install the steering column access cover (1).